**Abthorpe Old School**

**Audio amplifier equipment**

OVERALL

It is better to have 50% - 80% volume and adjust the input to suit.

INPUTS

1. Already wired to the ‘Bluetooth’ or Mic3/Aux input is a Bluetooth receiver, stuck at the left-hand- side of the amp. When on, there is a blue light. If you have not paired your Bluetooth device with this amp before, first press the centre of the adapter, then discover the “Esinkin BT adapter” on *your* device.
2. A trailing wire with a couple of phono connectors links to the ‘Aux’/’Line’ input
3. A microphone is connected to the MIC2 input – be sure the switch on the microphone is off (and the gain turned down) when not in use.

The amp is switched on at the right-hand side of the amp – a red indicator light should be on.

You should keep all input gain controls (little knobs) right down if that input is not being used.

Once you have a connection, adjust the treble and base tone controls to suit.

**SWITCH THE AMP OFF when you have finished.** Don’t bother trying to switch off the Bluetooth receiver.

Contact Eric Malcomson on 01327 857066 if you have any connection issues. He has a few adaptors for audio and video equipment to connect to the amp.

**WiFi access to the internet**

There is a permanently available WiFi access point called ‘Village Hall’ with no password. This link, and the wired link available in the hall and the small room, share the same network so be aware all devices connected can see each other. The link from the Village Hall is secure.